{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["劳务分包报价清单"],"not_rendered":{"external_links":3,"defined_names":5},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"劳务分包报价清单","index":0,"n_rows":142,"n_cols":8,"rows_kept":142,"merged":[[0,0,0,7],[1,0,1,7],[2,6,2,7],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,3,6],[3,7,4,7]],"flags":["formulas_cached_only"]}
["劳务分包报价清单"]
["项目名称：新福兴钙科技绿色新材料项目一期1#办公楼及宿舍、2#宿舍及食堂、3#厂房、外网及道路、零星签证劳务分包"]
[{"$nulls":6},"单位：人民币元"]
["序号","项目名称","项目特征描述","计量\n单位","合同单价","暂定工程造价",null,"备注"]
[{"$nulls":5},"工程量","合价"]
[1,"有保温隔热上人屋面","有保温隔热屋面 \n1.50厚C20细石混凝土保护层，内配HPB300,Φ6@150*150\n3.30厚挤塑聚苯乙烯泡沫塑料板\n4.4mm厚SBS改性沥青防水卷材\n5.50厚1：3水泥砂浆找平层\n6.钢筋混凝土屋面板","㎡",null,{"v":4470,"d":"4,470.00"},0]
[2,"新增混凝土楼梯及楼梯间屋面 （12-13*G-H轴  ）的旧结构拆除","1、切割混凝土屋面\n2、新增楼梯区域范围凿除    \n3、凿除混凝土块渣清运\n","项",null,{"v":1,"d":"1.00"},0]
[3,"二~四层楼面改造的旧结构拆除","1、切割混凝土楼板、屋面\n2、凿除混凝土块渣清运\n3、钢筋切割\n","项",null,{"v":1,"d":"1.00"},0]
[4,"新增中庭钢屋面的旧结构拆除","1、切割混凝土楼板、屋面\n2、凿除混凝土块渣清运\n","项",null,{"v":1,"d":"1.00"},0]
[5,"原结构预留钢筋人工切割","含切割人工 机具 辅耗材","项",null,{"v":1,"d":"1.00"},0]
[6,"10以内钢筋","现浇构钢筋\u007f\n1.钢筋种类、规格:HRB400 10以内 HRB335钢筋 10以内","t",null,{"v":27,"d":"27.00"},0]
[7,"10以上钢筋","现浇构件钢筋\u007f\n1.钢筋种类、规格:HRB400 10以上","t",null,{"v":6,"d":"6.00"},0]
[8,"C20垫层砼","基础垫层、车间地面垫层\u007f\n1.混凝土种类:泵送商品混凝土\n2.混凝土强度等级:C20，聚合物水泥混凝土","m3",null,{"v":63,"d":"63.00"},0]
[9,"C30砼","楼地面、直形墙、基础梁、矩形梁、有梁板、雨篷、直形楼梯\u007f\n1.混凝土种类:泵送普通商品混泥土\n2.混凝土强度等级:C30","m3",null,{"v":300,"d":"300.00"},0]
[10,"模板制安","所有 模板\u007f\n1.模板、支撑材质:胶合板 钢支撑","m2",null,{"v":1600,"d":"1,600.00"},0]
[11,"满堂架\n（支模）","超过3.6m层高计算，盘扣满堂支模架","m3",null,{"v":400,"d":"400.00"},0]
[12,"挖掘机挖沟槽、基坑","挖一般土方 \n1.土壤类别:一、二类土\n2.弃土运距:不弃土","m3",null,{"v":21100,"d":"21,100.00"},0]
[13,"回填土 夯实机夯实 槽、坑","回填方\u007f\n1.密实度:大于0.94\n2.填方材料品种:素土","m3",null,{"v":13965,"d":"13,965.00"},0]
[14,"钢承板","楼承板安装、边模安装","m2",null,{"v":100,"d":"100.00"},0]
[15,"屋面钢结构","主体钢结构\nQ355B钢板，Q355B型材；安装","t",null,{"v":5,"d":"5.00"},0]
[16,"剪力钉","焊接剪力钉","个",null,{"v":500,"d":"500.00"},0]
[17,"化学螺栓","化学螺栓：16*190","个",null,{"v":72,"d":"72.00"},0]
[18,"钻孔植筋（水钻取孔）",null,"个",null,{"v":36,"d":"36.00"},0]
[19,"喷射混凝土（砂浆）支护","喷射混凝土、水泥砂浆\u007f\n1.部位:基坑边坡\n2.厚度:100mm\n3.混凝土(砂浆)种类、强度等级:C25","m2",null,{"v":6000,"d":"6,000.00"},0]
[20,"坡面泄水管","1.钻排水孔                       2.安装Φ50PVC排水管 长度50公分","m",null,{"v":1500,"d":"1,500.00"},0]
[21,"支护\n砖地沟、明暗沟","1.截面300*300*120                       2.MU10砖砌排水沟","m",null,{"v":200,"d":"200.00"},0]
[22,"砖砌集水井","1.截面1000*1000*1000*240                       2.MU10砖砌集水井","座",null,{"v":4,"d":"4.00"},0]
[23,"土方运输道路","汽车运输道路 碎石铺设30cm厚\n50米长 6米宽 2条","项",null,{"v":1,"d":"1.00"},0]
[24,"基坑降水台班","排水、降水","项",null,{"v":1,"d":"1.00"},0]
[25,"基坑临边防护","Φ48钢管护栏，高度1.2米","项",null,{"v":1,"d":"1.00"},0]
[26,"降低效费",null,"项",null,{"v":1,"d":"1.00"},0]
[27,"避雷网安装(沿折板支架敷设) φ10热镀锌圆钢",null,"m",null,{"v":1940,"d":"1,940.00"},0]
[28,"利用柱内钢筋、基础粱钢筋做避雷引下线",null,"m",null,{"v":9677,"d":"9,677.00"},0]
[29,"接地母线 镀锌扁钢 40*4",null,"m",null,{"v":4551,"d":"4,551.00"},0]
[30,"接地极 镀锌扁钢 40*4",null,"根",null,{"v":20,"d":"20.00"},0]
[31,"配电房或弱电机房等预埋接地连接钢板",null,"根",null,{"v":20,"d":"20.00"},0]
[32,"接地电阻测试点",null,"处",null,{"v":16,"d":"16.00"},0]
[33,"局部等电位端子箱","100*100*6,接地预埋件位置标高为0.5m","个",null,{"v":208,"d":"208.00"},0]
[34,"总等电位端子箱",null,"台",null,{"v":10,"d":"10.00"},0]
[35,"接地装置",null,"系统",null,{"v":6,"d":"6.00"},0]
[36,"照明配电箱、电表箱、消防照明配电箱、接线箱",null,"台",null,{"v":75,"d":"75.00"},0]
[37,"设备配电箱",null,"台",null,{"v":7,"d":"7.00"},0]
[38,"户内配电箱",null,"台",null,{"v":145,"d":"145.00"},0]
[39,"桥架 ","CT-150x75、MR200X100 MR100X100","m",null,{"v":682,"d":"682.00"},0]
[40,"桥架 ","MR300X200 MR100X100\nCT-150x75","m",null,{"v":267,"d":"267.00"},0]
[41,"单管、双管LED灯","36W,~220V 层高不超3.6m\n安装部位：配电房、机房","个",null,{"v":44,"d":"44.00"},0]
[42,"吸顶灯(配LED灯)","12W ~220V 层高不超3.6m\n安装部位：雨棚、卫生间","个",null,{"v":32,"d":"32.00"},0]
[43,"LED投光灯","100-200W ~220V 层高15米以内\n安装部位：车间钢柱或顶棚","个",null,{"v":185,"d":"185.00"},0]
[44,"消防应急灯、指示灯",null,"个",null,{"v":584,"d":"584.00"},0]
[45,"开关、插座","三相五孔插座、86系列 ~16A 安全型、86系列 10A、Ex d IIC T6","个",null,{"v":145,"d":"145.00"},0]
[46,"镀锌钢管 DN50",null,"m",null,104.88,0]
[47,"镀锌钢管 DN100",null,"m",null,23.86,0]
[48,"防水套管 DN100",null,"m",null,{"v":4,"d":"4.00"},0]
[49,"配管","PC20、PC25、PC32、JDG20、JDG25","m",null,{"v":14360,"d":"14,360.00"},0]
[50,"配管","JDG32、JDG50","m",null,{"v":2200,"d":"2,200.00"},0]
[51,"配管","DN40","m",null,117.32,0]
[52,"空白面板、接线盒",null,"个",null,{"v":4992,"d":"4,992.00"},0]
[53,"金属软管",null,"根",null,{"v":459,"d":"459.00"},0]
[54,"50×5角铁","桥架支架、配电箱支架等","m",null,{"v":9844,"d":"9,844.00"},0]
[55,"电缆安装","50mm2以下的电缆安装","m",null,{"v":600,"d":"600.00"},0]
[56,"电线安装、应急照明电线安装","4mm2以下电线安装","m",null,{"v":36000,"d":"36,000.00"},0]
[57,"消防报警器",null,"m",null,{"v":258,"d":"258.00"},0]
[58,"防火堵洞（防火分区封堵）",null,"处",null,{"v":21,"d":"21.00"},0]
[59,"防火涂料 管道",null,"m2",null,{"v":205,"d":"205.00"},0]
[60,"自动投入装置系统调试（备用电源自动投入装置）","双电源配电箱调试","系统/台",null,{"v":9,"d":"9.00"},0]
[61,"自动投入装置系统调试（备用电源自动投入装置）","消防系统调试","系统/台",null,{"v":3,"d":"3.00"},0]
[62,"塑料直通雨水管及管件安装 U-PVC110、U-PVC160",null,"m",null,{"v":768,"d":"768.00"},0]
[63,"套管制作、安装","公称直径160mm以及100mm以内","个",null,{"v":379,"d":"379.00"},0]
[64,"普通雨水斗公称直径100mm以内",null,"个",null,{"v":46,"d":"46.00"},0]
[65,"管道消音",null,"m",null,{"v":516,"d":"516.00"},0]
[66,"阻火圈安装",null,"个",null,{"v":106,"d":"106.00"},0]
[67,"PVC 排水管","室内塑料排水管（粘接） \n外径 100mm以内）","m",null,{"v":1192.4,"d":"1,192.40"},0]
[68,"PVC 排水管","室内塑料排水管（粘接） \n外径 150mm以内）","m",null,{"v":212,"d":"212.00"},0]
[69,"管道消音","室内塑料排水管 隔音棉安装（粘接） \n外径 100mm~150mm以内）","m",null,{"v":1200,"d":"1,200.00"},0]
[70,"打洞（孔）","金刚钻孔 堵洞\n混凝土楼板 厚度100mm~120mm 公称直径150mm~20mm以内","个",null,{"v":276,"d":"276.00"},0]
[71,"阻火圈安装","梁板下安装(公称直径100mm以内)","个",null,{"v":140,"d":"140.00"},0]
[72,"大、小便器、洗脸盆及其他洁具","蹲式大便器 液压脚踏式冲洗阀","套",null,{"v":31,"d":"31.00"},0]
[73,"给、排水附(配)件","地面扫除口安装(公称直径100mm以内)","个",null,{"v":4,"d":"4.00"},0]
[74,"PPR给水管","(1)连接形式:热熔\n(2)安装部位:室内\n(3)材质、规格:DN80以上-DN150以内","m",null,{"v":200,"d":"200.00"},0]
[75,"PPR给水管","(1)连接形式:热熔\n(2)安装部位:室内\n(3)材质、规格:DN80以下","m",null,{"v":800,"d":"800.00"},0]
[76,"管道保温","热水管道保温（管束） 外径 20mm~50mm以内 保温厚度30mm）","m",null,{"v":600,"d":"600.00"},0]
[77,"管道保温","热水管道保温（管束） 外径 65mm~100mm以内 保温厚度40mm）","m",null,{"v":200,"d":"200.00"},0]
[78,"管件","(1)规格、型号:三通、弯头等管件（包含变径，以大头为准） DN50-DN20\n(2)连接形式：热熔","个",null,{"v":20,"d":"20.00"},0]
[79,"管件","(1)规格、型号:三通、弯头等管件（包含变径，以大头为准） DN50-DN100\n(2)连接形式：热熔","个",null,{"v":100,"d":"100.00"},0]
[80,"管件","(1)规格、型号:三通、弯头等管件（包含变径，以大头为准） DN50-DN20\n(2)连接形式：热熔","个",null,{"v":200,"d":"200.00"},0]
[81,"法兰阀门","(1)连接形式:法兰\n(2)材质:碳钢\n(3)规格、压力等级:DN100\n1.6MPA（包含闸阀、蝶阀、电磁阀、倒流防止器、软接头等同规格附件）","个",null,{"v":2,"d":"2.00"},0]
[82,"法兰阀门","(1)连接形式:法兰\n(2)材质:碳钢\n(3)规格、压力等级:DN80\n1.6MPA（包含闸阀、蝶阀、电磁阀、倒流防止器、软接头等同规格附件）","个",null,{"v":20,"d":"20.00"},0]
[83,"法兰阀门","(1)连接形式:法兰\n(2)材质:碳钢\n(3)规格、压力等级:DN65、\n1.6MPA（包含闸阀、蝶阀、电磁阀、倒流防止器、软接头等同规格附件）","个",null,{"v":20,"d":"20.00"},0]
[84,"螺纹阀门","螺纹阀门安装(公称直径25mm以内)","个",null,{"v":33,"d":"33.00"},0]
[85,"螺纹阀门","(1)连接形式:螺纹\n(2)材质:碳钢\n(3)规格、压力等级:DN50、DN40、DN20\n1.6MPA","个",null,{"v":60,"d":"60.00"},0]
[86,"压力仪表","(1)名称、规格:压力表 Y-100 0~1.6Mpa\n(2)连接形式:按设计规范要求","台",null,{"v":31,"d":"31.00"},0]
[87,"套管","套管制作、安装公称直径150mm~20mm以内","个",null,{"v":100,"d":"100.00"},0]
[88,"阻火圈安装","梁板下安装(公称直径100mm~20mm以内)","个",null,{"v":120,"d":"120.00"},0]
[89,"水泵","冷热水生活泵","套",null,{"v":12,"d":"12.00"},0]
[90,"水泵控制柜","冷热水生活水泵控制柜","套",null,{"v":4,"d":"4.00"},0]
[91,"墙面开槽及修补","(1)材质:碳钢\n(2)规格:DN20-DN50","m",null,{"v":70,"d":"70.00"},0]
[92,"消火栓钢管","(1)连接形式:沟槽连接\n(2)安装部位:室内\n(3)材质、规格:内外热镀锌钢管DN150","m",null,{"v":2000,"d":"2,000.00"},0]
[93,"消火栓钢管","(1)连接形式:沟槽连接\n(2)安装部位:室内\n(3)材质、规格:内外热镀锌钢管DN100","m",null,{"v":540,"d":"540.00"},0]
[94,"消火栓钢管","(1)连接形式:沟槽连接\n(2)安装部位:室内\n(3)材质、规格:内外热镀锌钢管DN65（超高）\n(4)压力试验及冲洗设计要求:水压试验、水冲洗","m",null,{"v":800,"d":"800.00"},0]
[95,"管道刷油","(1)油漆品种:醇酸磁漆\n(2)涂刷遍数、漆膜厚度:两遍","m2",null,{"v":1499,"d":"1,499.00"},0]
[96,"管道支架刷油","(1)结构类型:管道支架刷油\n(2)除锈级别:除轻锈\n(3)油漆品种:醇酸磁漆","m",null,{"v":4730,"d":"4,730.00"},0]
[97,"套管","(1)材质:碳钢\n(2)规格:介质管道DN150\n(3)填料材质:油麻、密封油膏等\n(4)名称、类型:穿楼面套管","个",null,{"v":86,"d":"86.00"},0]
[98,"沟槽阀门","(1)连接形式:沟槽\n(2)材质:碳钢\n(3)规格、压力等级:DN100 1.6MPA\n(4)类型:蝶阀","个",null,{"v":57,"d":"57.00"},0]
[99,"法兰","(1)材质:钢制法兰\n(2)连接形式:法兰连接\n(3)规格、压力等级:DN150","副",null,{"v":57,"d":"57.00"},0]
[100,"室内消火栓箱","安装方式：明装","套",null,{"v":131,"d":"131.00"},0]
[101,"灭火器（磷酸铵盐干粉灭火器（MF/ABC6)","安装方式：明装","具",null,{"v":258,"d":"258.00"},0]
[102,"水灭火控制装置调试","(1)系统形式:水灭火控制装置调试(消火栓灭火系统)","点",null,{"v":131,"d":"131.00"},0]
[103,"抗震支吊架","侧向DN100以下","套",null,{"v":50,"d":"50.00"},0]
[104,"抗震支吊架","侧向DN150","套",null,{"v":160,"d":"160.00"},0]
[105,"管道挖土方","(1)挖基槽土方\n(2)深度1.0m内，DN32-DN200","m",null,478.85,0]
[106,"管道回填土方","(1)回填基槽土方\n(2)深度1.0m内，DN32-DN200","m",null,{"v":40,"d":"40.00"},0]
[107,"金刚钻取孔","(1)规格:介质管道DN32-DN250\n(2)名称、类型:穿地梁套管及楼板等\n(3)金刚钻取孔","个",null,{"v":20,"d":"20.00"},0]
[108,"防火阀","常开，70摄氏度 感温关闭\n使用部位：电房","套",null,{"v":7,"d":"7.00"},0]
[109,"排风机","P1-P7 DKT15 \n使用部位：电房","套",null,{"v":7,"d":"7.00"},0]
[110,"防雨百叶1","排风机防雨百叶 1500*1500\n其他防雨百叶2500*1500+3000*500+500*250+1600*500","套",null,{"v":14,"d":"14.00"},0]
[111,"天花管道式排气扇","使用部位：卫生间","套",null,{"v":12,"d":"12.00"},0]
[112,"风管","800*320、1200*500、800*400、15000*500、320*200、500*250、1600*500、","m",null,{"v":92,"d":"92.00"},0]
[113,"外墙及内墙面取孔","取孔含封堵","个",null,{"v":19,"d":"19.00"},0]
[114,"高空措施费","登高车、脚手架 使用包干费","项",null,{"v":1,"d":"1.00"},0]
[115,"PE给水管","(1)连接形式:热熔\n(2)安装部位:室外\n(3)材质、规格:DN200 1.6mpa","m",null,{"v":1400,"d":"1,400.00"},0]
[116,"PE给水管","(1)连接形式:热熔\n(2)安装部位:室外\n(3)材质、规格:DN100 1.6mpa","m",null,{"v":200,"d":"200.00"},0]
[117,"管件","(1)规格、型号:弯头、三通、变径 \nDN100、DN200\n(2)连接形式：热熔","个",null,{"v":30,"d":"30.00"},0]
[118,"法兰阀门","(1)连接形式:法兰\n(2)材质:碳钢\n(3)规格、压力等级:DN200 1.6MPA\n(4)类型:闸阀","套",null,{"v":4,"d":"4.00"},0]
[119,"水表","(1)连接形式:法兰\n(2)安装部位:室外\n(3)材质、规格:DN200普通水表","个",null,{"v":1,"d":"1.00"},0]
[120,"倒流防止器","(1)连接形式:法兰\n(2)安装部位:室外\n(3)材质、规格:DN200","套",null,{"v":1,"d":"1.00"},0]
[121,"法兰","(1)连接形式:法兰\n(2)安装部位:室外\n(3)材质、规格:DN100~200 1.6mpa","副",null,{"v":16,"d":"16.00"},0]
[122,"室外消火栓","(1)连接形式:法兰\n(2)安装部位:室外\n(3)材质、规格:DN100 SS100/65-1.6","套",null,{"v":12,"d":"12.00"},0]
[123,"双壁波纹管","(1)连接形式:承插式\n(2)安装部位:室外\n(3)材质、规格:HDPE1000 环刚度SN8","m",null,{"v":200,"d":"200.00"},0]
[124,"双壁波纹管","(1)连接形式:承插式\n(2)安装部位:室外\n(3)材质、规格:HDPE800 环刚度SN8","m",null,{"v":200,"d":"200.00"},0]
[125,"双壁波纹管","(1)连接形式:承插式\n(2)安装部位:室外\n(3)材质、规格:HDPE600 环刚度SN8","m",null,{"v":100,"d":"100.00"},0]
[126,"双壁波纹管","(1)连接形式:承插式\n(2)安装部位:室外\n(3)材质、规格:HDPE500 环刚度SN8","m",null,{"v":250,"d":"250.00"},0]
[127,"双壁波纹管","(1)连接形式:承插式\n(2)安装部位:室外\n(3)材质、规格:HDPE400 环刚度SN8","m",null,{"v":300,"d":"300.00"},0]
[128,"双壁波纹管","(1)连接形式:承插式\n(2)安装部位:室外\n(3)材质、规格:HDPE300 环刚度SN8","m",null,{"v":900,"d":"900.00"},0]
[129,"消火栓管","(1)连接形式:电熔\n(2)安装部位:室外\n(3)材质、规格:钢丝网骨架复合管DN200 1.6mpa","m",null,{"v":1205,"d":"1,205.00"},0]
[130,"管件","(1)规格、型号:直接、弯头 三通 DN200\n(2)连接形式：电熔","个",null,{"v":180,"d":"180.00"},0]
[131,"砖砌雨水井、污水井、消防阀门井","（1）Ф700圆形收口井  H=1600\n（2）C10混凝土垫层\n（3）MU10级砖M10水泥砂浆井壁\n（4）D700、D1000重型球墨铸铁井盖、井座安装","座",null,{"v":33,"d":"33.00"},0]
[132,"砖砌雨水井","（1）Ф1250圆形收口井  H=2000\n（2）C10混凝土垫层\n（3）MU10级砖M10水泥砂浆井壁\n（4）D1250重型球墨铸铁井盖、井座安装","座",null,{"v":6,"d":"6.00"},0]
[133,"砖砌雨水井","（1）Ф1500圆形收口井  H=2200、H=2500、H=3500、H=4500\n（2）C10混凝土垫层\n（3）MU10级砖M10水泥砂浆井壁\n（4）D1500重型球墨铸铁井盖、井座安装","座",null,{"v":3,"d":"3.00"},0]
[134,"室外明沟","混凝土浇倒","m",null,{"v":1000,"d":"1,000.00"},0]
[135,"室外道路","混凝土路面：20公分、压纹","m2",null,{"v":14500,"d":"14,500.00"},0]
[136,"措施费用（含人员进退场、临时设施费、大型机械进出场费、临时水电敷设、现场安全围档护栏等费用）",null,"项",null,{"v":1,"d":"1.00"},0]
[null,null,"小计",{"$nulls":3},0]